;
; Asterisk Builtin mini-HTTP server
;
;
[general]
;
; Whether HTTP interface is enabled or not.  Default is no.
;
;enabled=yes
;
; Whether Asterisk should serve static content from http-static
; Default is no.
;
;enablestatic=yes
;
; Address to bind to.  Default is 0.0.0.0
;
bindaddr=127.0.0.1
;
; Port to bind to (default is 8088)
;
bindport=8088
;
; Prefix allows you to specify a prefix for all requests
; to the server.  The default is "asterisk" so that all
; requests must begin with /asterisk
;
;prefix=asterisk
