;
; Automatically generated from ../channels/chan_oss.c
;

[general]
    ; General config options, with default values shown.
    ; You should use one section per device, with [general] being used
    ; for the first device and also as a template for other devices.
    ;
    ; All but 'debug' can go also in the device-specific sections.
    ;
    ; debug = 0x0		; misc debug flags, default is 0

    ; Set the device to use for I/O
    ; device = /dev/dsp

    ; Optional mixer command to run upon startup (e.g. to set
    ; volume levels, mutes, etc.
    ; mixer =

    ; Software mic volume booster (or attenuator), useful for sound
    ; cards or microphones with poor sensitivity. The volume level
    ; is in dB, ranging from -20.0 to +20.0
    ; boost = n			; mic volume boost in dB

    ; Set the callerid for outgoing calls
    ; callerid = John Doe <555-1234>

    ; autoanswer = no		; no autoanswer on call
    ; autohangup = yes		; hangup when other party closes
    ; extension = s		; default extension to call
    ; context = default		; default context for outgoing calls
    ; language = ""		; default language

    ; If you set overridecontext to 'yes', then the whole dial string
    ; will be interpreted as an extension, which is extremely useful
    ; to dial SIP, IAX and other extensions which use the '@' character.
    ; The default is 'no' just for backward compatibility, but the
    ; suggestion is to change it.
    ; overridecontext = no	; if 'no', the last @ will start the context
				; if 'yes' the whole string is an extension.

    ; low level device parameters in case you have problems with the
    ; device driver on your operating system. You should not touch these
    ; unless you know what you are doing.
    ; queuesize = 10		; frames in device driver
    ; frags = 8			; argument to SETFRAGMENT

[card1]
    ; device = /dev/dsp1	; alternate device

