;
; IAX2 Provisioning Information
;
; Contains provisioning information for templates and for specific service
; entries.
;
; Templates provide a group of settings from which provisioning takes place.
; A template may be based upon any template that has been specified before
; it.  If the template that an entry is based on is not specified then it is
; presumed to be 'default' (unless it is the first of course).  
;
; Templates which begin with 'si-' are used for provisioning units with
; specific service identifiers.  For example the entry "si-000364000126"
; would be used when the device with the corresponding service identifier of
; "000364000126" attempts to register or make a call.
;
[default]
;
; The port number the device should use to bind to.  The default is 4569.
;
;port=4569
;
; server is our PRIMARY server for registration and placing calls
;
;server=192.168.69.3
;
; altserver is the BACKUP server for registration and placing calls in the
; event the primary server is unavailable.
;
;altserver=192.168.69.4
;
; port is the port number to use for IAX2 outbound.  The connections to the
; server and altserver -- default is of course 4569.
;serverport=4569
;
; language is the preferred language for the device
;
;language=en
;
; codec is the requested codec.  The iaxy supports ulaw and adpcm
;
codec=ulaw
;
; flags is a comma separated list of flags which the device should
; use and may contain any of the following keywords:
;
;  "register"  - Register with server
;  "secure"    - Do not accept calls / provisioning not originated by the server
;  "heartbeat" - Generate status packets on port 9999 sent to 255.255.255.255
;  "debug"     - Output extra debugging to port 9999
;
;  Note that use can use += and -= to adjust parameters
;
flags=register,heartbeat
;
; See doc/README.tos for a description of this parameter.
;tos=ef
;
; Example iaxy provisioning
;
;[si-000364000126]
;user=iaxy
;pass=bitsy
;flags += debug

;[si-000364000127]
;user=iaxy2
;pass=bitsy2
;template=si-000364000126
;flags += debug

;
;[*]
;
;  If specified, the '*' provisioning is used for all devices which do not
;  have another provisioning entry within the file.  If unspecified, no
;  provisioning will take place for devices which have no entry.  DO NOT
;  USE A '*' PROVISIONING ENTRY UNLESS YOU KNOW WHAT YOU'RE DOING.
;
;template=default

