;
; Asterisk Builtin mini-HTTP server
;
;
[general]
;
; Whether HTTP interface is enabled or not.  Default is no.
;
;enabled=yes
;
; Whether Asterisk should serve static content from http-static
; Default is no.
;
;enablestatic=yes
;
; Address to bind to.  Default is 0.0.0.0
;
bindaddr=127.0.0.1
;
; Port to bind to (default is 8088)
;
bindport=8088
;
; Prefix allows you to specify a prefix for all requests
; to the server.  The default is "asterisk" so that all
; requests must begin with /asterisk
;
;prefix=asterisk

; The post_mappings section maps URLs to real paths on the filesystem.  If a
; POST is done from within an authenticated manager session to one of the
; configured POST mappings, then any files in the POST will be placed in the
; configured directory.
;
;[post_mappings]
;
; In this example, if the prefix option is set to "asterisk", then using the
; POST URL: /asterisk/uploads will put files in /var/lib/asterisk/uploads/.
;uploads = /var/lib/asterisk/uploads/
;
