//
// Example AEL config file
//
//
// Static extension configuration file, used by
// the pbx_ael module. This is where you configure all your 
// inbound and outbound calls in Asterisk. 
// 
// This configuration file is reloaded 
// - With the "ael reload" command in the CLI
// - With the "reload" command (that reloads everything) in the CLI

// The "Globals" category contains global variables that can be referenced
// in the dialplan by using the GLOBAL dialplan function:
//  ${GLOBAL(VARIABLE)} 
// ${${GLOBAL(VARIABLE)}} or ${text${GLOBAL(VARIABLE)}} or any hybrid
// Unix/Linux environmental variables are reached with the ENV dialplan
// function: ${ENV(VARIABLE)}
//

globals {
	CONSOLE="Console/dsp"; 		// Console interface for demo
	//CONSOLE=Zap/1
	//CONSOLE=Phone/phone0
	IAXINFO=guest;				// IAXtel username/password
	//IAXINFO="myuser:mypass";
	TRUNK="Zap/g2";					// Trunk interface
	//
	// Note the 'g2' in the TRUNK variable above. It specifies which group (defined
	// in chan_dahdi.conf) to dial, i.e. group 2, and how to choose a channel to use in
	// the specified group. The four possible options are:
	//
	// g: select the lowest-numbered non-busy Zap channel
	//    (aka. ascending sequential hunt group).
	// G: select the highest-numbered non-busy Zap channel
	//    (aka. descending sequential hunt group).
	// r: use a round-robin search, starting at the next highest channel than last
	//    time (aka. ascending rotary hunt group).
	// R: use a round-robin search, starting at the next lowest channel than last
	//    time (aka. descending rotary hunt group).
	//
	TRUNKMSD=1;					// MSD digits to strip (usually 1 or 0)
	//TRUNK=IAX2/user:pass@provider
};

//
// Any category other than "General" and "Globals" represent 
// extension contexts, which are collections of extensions.  
//
// Extension names may be numbers, letters, or combinations
// thereof. If an extension name is prefixed by a '_'
// character, it is interpreted as a pattern rather than a
// literal.  In patterns, some characters have special meanings:
//
//   X - any digit from 0-9
//   Z - any digit from 1-9
//   N - any digit from 2-9
//   [1235-9] - any digit in the brackets (in this example, 1,2,3,5,6,7,8,9)
//   . - wildcard, matches anything remaining (e.g. _9011. matches 
//	anything starting with 9011 excluding 9011 itself)
//   ! - wildcard, causes the matching process to complete as soon as
//       it can unambiguously determine that no other matches are possible
//
// For example the extension _NXXXXXX would match normal 7 digit dialings, 
// while _1NXXNXXXXXX would represent an area code plus phone number
// preceded by a one.
//
// Each step of an extension is ordered by priority, which must
// always start with 1 to be considered a valid extension.  The priority
// "next" or "n" means the previous priority plus one, regardless of whether
// the previous priority was associated with the current extension or not.
// The priority "same" or "s" means the same as the previously specified
// priority, again regardless of whether the previous entry was for the
// same extension.  Priorities may be immediately followed by a plus sign
// and another integer to add that amount (most useful with 's' or 'n').  
// Priorities may then also have an alias, or label, in 
// parenthesis after their name which can be used in goto situations
//
// Contexts contain several lines, one for each step of each
// extension, which can take one of two forms as listed below,
// with the first form being preferred.  One may include another
// context in the current one as well, optionally with a
// date and time.  Included contexts are included in the order
// they are listed.
//
//context name {
//	exten-name => {
//		application(arg1,arg2,...);
//
// 	Timing list for includes is 
//
//   <time range>|<days of week>|<days of month>|<months>
//
//	includes { 
//		daytime|9:00-17:00|mon-fri|*|*;
//      };
//
// 	ignorepat can be used to instruct drivers to not cancel dialtone upon
// 	receipt of a particular pattern.  The most commonly used example is
// 	of course '9' like this:
//
//	ignorepat => 9;
//
// 	so that dialtone remains even after dialing a 9.
//};


//
// Sample entries for extensions.conf
//
//
context ael-dundi-e164-canonical {
	//
	// List canonical entries here
	//
	// 12564286000 => &ael-std-exten(6000,IAX2/foo);
	// _125642860XX => Dial(IAX2/otherbox/${EXTEN:7});
};

context ael-dundi-e164-customers {
	//
	// If you are an ITSP or Reseller, list your customers here.
	//
	//_12564286000 => Dial(SIP/customer1);
	//_12564286001 => Dial(IAX2/customer2);
};

context ael-dundi-e164-via-pstn {
	//
	// If you are freely delivering calls to the PSTN, list them here
	//
	//_1256428XXXX => Dial(Zap/g2/${EXTEN:7}); // Expose all of 256-428 
	//_1256325XXXX => Dial(Zap/g2/${EXTEN:7}); // Ditto for 256-325
};

context ael-dundi-e164-local {
	//
	// Context to put your dundi IAX2 or SIP user in for
	// full access
	//
	includes {
	 ael-dundi-e164-canonical;
	 ael-dundi-e164-customers;
	 ael-dundi-e164-via-pstn;
	};
};

context ael-dundi-e164-switch {
	//
	// Just a wrapper for the switch
	//
	
	switches { 
		DUNDi/e164;
	};
};

context ael-dundi-e164-lookup {
	//
	// Locally to lookup, try looking for a local E.164 solution
	// then try DUNDi if we don't have one.
	//
	includes {
		ael-dundi-e164-local;
		ael-dundi-e164-switch;
	};
	//
};

//
// DUNDi can also be implemented as a Macro instead of using 
// the Local channel driver. 
//
macro ael-dundi-e164(exten) {
//
// ARG1 is the extension to Dial
//
	goto ${exten}|1;
	return;
};

//
// Here are the entries you need to participate in the IAXTEL
// call routing system.  Most IAXTEL numbers begin with 1-700, but
// there are exceptions.  For more information, and to sign
// up, please go to www.gnophone.com or www.iaxtel.com
//
context ael-iaxtel700 {
	_91700XXXXXXX => Dial(IAX2/${IAXINFO}@iaxtel.com/${EXTEN:1}@iaxtel);
};

//
// The SWITCH statement permits a server to share the dialplan with
// another server. Use with care: Reciprocal switch statements are not
// allowed (e.g. both A -> B and B -> A), and the switched server needs
// to be on-line or else dialing can be severly delayed.
//
context ael-iaxprovider {
	switches {
	// IAX2/user:[key]@myserver/mycontext;
	};
};

context ael-trunkint {
	//
	// International long distance through trunk
	//
	includes {
		ael-dundi-e164-lookup;
	};
	_9011. => {
		&ael-dundi-e164(${EXTEN:4});
		Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
	};
};

context ael-trunkld {
	//
	// Long distance context accessed through trunk
	//
	includes {
		ael-dundi-e164-lookup;
	};
	_91NXXNXXXXXX => {
		&ael-dundi-e164(${EXTEN:1});
		Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
	};
};

context ael-trunklocal {
	//
	// Local seven-digit dialing accessed through trunk interface
	//
	_9NXXXXXX => {
		Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
	};
};

context ael-trunktollfree {
	//
	// Long distance context accessed through trunk interface
	//
	
	_91800NXXXXXX => Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
	_91888NXXXXXX => Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
	_91877NXXXXXX => Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
	_91866NXXXXXX => Dial(${TRUNK}/${EXTEN:${TRUNKMSD}});
};

context ael-international {
	//
	// Master context for international long distance
	//
	ignorepat => 9;
	includes {
		ael-longdistance;
		ael-trunkint;
	};
};

context ael-longdistance {
	//
	// Master context for long distance
	//
	ignorepat => 9;
	includes {
		ael-local;
		ael-trunkld;
	};
};

context ael-local {
	//
	// Master context for local, toll-free, and iaxtel calls only
	//
	ignorepat => 9;
	includes {
		ael-default;
		ael-trunklocal;
		ael-iaxtel700;
		ael-trunktollfree;
		ael-iaxprovider;
	};
};

//
// You can use an alternative switch type as well, to resolve
// extensions that are not known here, for example with remote 
// IAX switching you transparently get access to the remote
// Asterisk PBX
// 
// switch => IAX2/user:password@bigserver/local
//
// An "lswitch" is like a switch but is literal, in that
// variable substitution is not performed at load time
// but is passed to the switch directly (presumably to
// be substituted in the switch routine itself)
//
// lswitch => Loopback/12${EXTEN}@othercontext
//
// An "eswitch" is like a switch but the evaluation of
// variable substitution is performed at runtime before
// being passed to the switch routine.
//
// eswitch => IAX2/context@${CURSERVER}


macro ael-std-exten-ael( ext , dev ) {
        Dial(${dev}/${ext},20);
        switch(${DIALSTATUS}) {
        case BUSY:
                Voicemail(${ext},b);
                break;
        default:
                Voicemail(${ext},u);
        };
        catch a {
                VoiceMailMain(${ext});
                return;
        };
	return;
};

context ael-demo {
	s => {
		Wait(1);
		Answer();
		Set(TIMEOUT(digit)=5);
		Set(TIMEOUT(response)=10);
restart:
		Background(demo-congrats);
instructions:
		for (x=0; ${x} < 3; x=${x} + 1) {
			Background(demo-instruct);
			WaitExten();
		};
	};
	2 => {
		Background(demo-moreinfo);
		goto s|instructions;
	};
	3 => {
		Set(LANGUAGE()=fr);
		goto s|restart;
	};
	1000 => {
		goto ael-default|s|1;
	};
	500 => {
		Playback(demo-abouttotry);
		Dial(IAX2/guest@misery.digium.com/s@default);
		Playback(demo-nogo);
		goto s|instructions;
	};
	600 => {
		Playback(demo-echotest);
		Echo();
		Playback(demo-echodone);
		goto s|instructions;
	};
	_1234 => &ael-std-exten-ael(${EXTEN}, "IAX2");
	8500 => {
		VoicemailMain();
		goto s|instructions;
	};
	# => {
		Playback(demo-thanks);
		Hangup();
	};
	t => goto #|1;
	i => Playback(invalid);
};


//
// If you wish to use AEL for your default context, remove it
// from extensions.conf (or change its name or comment it out)
// and then uncomment the one here.
//

context ael-default {

// By default we include the demo.  In a production system, you 
// probably don't want to have the demo there.

	includes {
		ael-demo;
	};
//
// Extensions like the two below can be used for FWD, Nikotel, sipgate etc.
// Note that you must have a [sipprovider] section in sip.conf whereas
// the otherprovider.net example does not require such a peer definition
//
//_41X. => Dial(SIP/${EXTEN:2}@sipprovider,,r);
//_42X. => Dial(SIP/user:passwd@${EXTEN:2}@otherprovider.net,30,rT);

// Real extensions would go here. Generally you want real extensions to be
// 4 or 5 digits long (although there is no such requirement) and start with a
// single digit that is fairly large (like 6 or 7) so that you have plenty of
// room to overlap extensions and menu options without conflict.  You can alias
// them with names, too, and use global variables

// 6245  => {
//		hint(SIP/Grandstream1&SIP/Xlite1,Joe Schmoe); // Channel hints for presence
// 		Dial(SIP/Grandstream1,20,rt);                 // permit transfer
//        Dial(${HINT}/5245},20,rtT);                    // Use hint as listed
//        switch(${DIALSTATUS}) {
//        case BUSY:
//                Voicemail(6245,b);
//				return;
//        default:
//                Voicemail(6245,u);
//				return;
//        };
//       };

// 6361 => Dial(IAX2/JaneDoe,,rm);                // ring without time limit
// 6389 => Dial(MGCP/aaln/1@192.168.0.14);
// 6394 => Dial(Local/6275/n);                    // this will dial ${MARK}

// 6275 => &ael-stdexten(6275,${MARK});           // assuming ${MARK} is something like Zap/2
// mark => goto 6275|1;                          // alias mark to 6275
// 6536 => &ael-stdexten(6236,${WIL});            // Ditto for wil
// wil  => goto 6236|1;
//
// Some other handy things are an extension for checking voicemail via
// voicemailmain
//
// 8500 => {
//			VoicemailMain();
//			Hangup();
//	       };
//
// Or a conference room (you'll need to edit meetme.conf to enable this room)
//
// 8600 => Meetme(1234);
//
// Or playing an announcement to the called party, as soon it answers
//
// 8700 => Dial(${MARK},30,A(/path/to/my/announcemsg))
//
// For more information on applications, just type "show applications" at your
// friendly Asterisk CLI prompt.
//
// 'show application <command>' will show details of how you
// use that particular application in this file, the dial plan. 
//
}
