#!/bin/sh
#
#	$Id: IPaddr2.in,v 1.24 2006/08/09 13:01:54 lars Exp $
#
#       OCF Resource Agent compliant IPaddr2 script.
#
# 	Based on work by Tuomo Soini, ported to the OCF RA API by Lars
# 	Marowsky-Brée. Implements Cluster Alias IP functionality too.
#
#	Cluster Alias IP cleanup, fixes and testing by Michael Schwartzkopff
#
#
# Copyright (c) 2003 Tuomo Soini
# Copyright (c) 2004-2006 SUSE LINUX AG, Lars Marowsky-Brée
#                    All Rights Reserved.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of version 2 of the GNU General Public License as
# published by the Free Software Foundation.
#
# This program is distributed in the hope that it would be useful, but
# WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
#
# Further, this software is distributed without any warranty that it is
# free of the rightful claim of any third person regarding infringement
# or the like.  Any license provided herein, whether implied or
# otherwise, applies only to this software file.  Patent licenses, if
# any, provided herein do not apply to combinations of this program with
# other software, or any other product whatsoever.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write the Free Software Foundation,
# Inc., 59 Temple Place - Suite 330, Boston MA 02111-1307, USA.
#
#


# TODO: 
# - There ought to be an ocf_run_cmd function which does all logging,
#   timeout handling etc for us
# - Make this the standard IP address agent on Linux; the other
#   platforms simply should ignore the additional parameters OR can use
#   the legacy heartbeat resource script...
# - Check LVS <-> clusterip incompatibilities.
#
#	OCF parameters are as below
#	OCF_RESKEY_ip
#	OCF_RESKEY_broadcast
#	OCF_RESKEY_nic
#	OCF_RESKEY_cidr_netmask
#	OCF_RESKEY_iflabel
#	OCF_RESKEY_mac
#	OCF_RESKEY_clusterip_hash
#	OCF_RESKEY_arp_interval
#	OCF_RESKEY_arp_count
#	OCF_RESKEY_arp_bg
#	OCF_RESKEY_arp_mac
#
#	OCF_RESKEY_CRM_meta_clone
#	OCF_RESKEY_CRM_meta_clone_max


#######################################################################
# Initialization:

. ${OCF_ROOT}/resource.d/heartbeat/.ocf-shellfuncs

SENDARP=$HA_BIN/send_arp
FINDIF=$HA_BIN/findif
VLDIR=$HA_RSCTMP/IPaddr
SENDARPPIDDIR=$HA_RSCTMP/send_arp
CIP_lockfile=$HA_RSCTMP/IPaddr2-CIP-${OCF_RESKEY_ip}

#######################################################################

meta_data() {
	cat <<END
<?xml version="1.0"?>
<!DOCTYPE resource-agent SYSTEM "ra-api-1.dtd">
<resource-agent name="IPaddr2">
<version>1.0</version>

<longdesc lang="en">
This Linux-specific resource manages IP alias IP addresses.
It can add an IP alias, or remove one.
In addition, it can implement Cluster Alias IP functionality
if invoked as a clone resource.
</longdesc>

<shortdesc lang="en">Manages virtual IPv4 addresses</shortdesc>

<parameters>
<parameter name="ip" unique="1" required="1">
<longdesc lang="en">
The IPv4 address to be configured in dotted quad notation, for example
"192.168.1.1".
</longdesc>
<shortdesc lang="en">IPv4 address</shortdesc>
<content type="string" default="" />
</parameter>
<parameter name="nic" unique="0">
<longdesc lang="en">
The base network interface on which the IP address will be brought
online. 

If left empty, the script will try and determine this from the
routing table.

Do NOT specify an alias interface in the form eth0:1 or anything here;
rather, specify the base interface only.

</longdesc>
<shortdesc lang="en">Network interface</shortdesc>
<content type="string" default="eth0"/>
</parameter>

<parameter name="cidr_netmask">
<longdesc lang="en">
The netmask for the interface in CIDR format
(e.g., 24 and not 255.255.255.0)

If unspecified, the script will also try to determine this from the
routing table.
</longdesc>
<shortdesc lang="en">CIDR netmask</shortdesc>
<content type="string" default=""/>
</parameter>

<parameter name="broadcast">
<longdesc lang="en">
Broadcast address associated with the IP. If left empty, the script will
determine this from the netmask.
</longdesc>
<shortdesc lang="en">Broadcast address</shortdesc>
<content type="string" default=""/>
</parameter>

<parameter name="iflabel">
<longdesc lang="en">
You can specify an additional label for your IP address here.
This label is appended to your interface name.
If a label is specified in nic name, this parameter has no effect.
</longdesc>
<shortdesc lang="en">Interface label</shortdesc>
<content type="string" default=""/>
</parameter>

<parameter name="lvs_support">
<longdesc lang="en">
Enable support for LVS Direct Routing configurations. In case a IP
address is stopped, only move it to the loopback device to allow the
local node to continue to service requests, but no longer advertise it
on the network.
</longdesc>
<shortdesc lang="en">Enable support for LVS DR</shortdesc>
<content type="boolean" default="false"/>
</parameter>

<parameter name="mac">
<longdesc lang="en">
Set the interface MAC address explicitly. Currently only used in case of
the Cluster IP Alias. Leave empty to chose automatically.

</longdesc>
<shortdesc lang="en">Cluster IP MAC address</shortdesc>
<content type="string" default=""/>
</parameter>

<parameter name="clusterip_hash">
<longdesc lang="en">
Specify the hashing algorithm used for the Cluster IP functionality.

</longdesc>
<shortdesc lang="en">Cluster IP hashing function</shortdesc>
<content type="string" default="sourceip-sourceport-destport"/>
</parameter>

<parameter name="arp_interval">
<longdesc lang="en">
Specify the interval between unsolicited ARP packets in milliseconds.
</longdesc>
<shortdesc lang="en">ARP packet interval in ms</shortdesc>
<content type="integer" default="200"/>
</parameter>

<parameter name="arp_count">
<longdesc lang="en">
Number of unsolicited ARP packets to send.
</longdesc>
<shortdesc lang="en">ARP packet count</shortdesc>
<content type="integer" default="5"/>
</parameter>

<parameter name="arp_bg">
<longdesc lang="en">
Whether or not to send the arp packets in the background.
</longdesc>
<shortdesc lang="en">ARP from background</shortdesc>
<content type="string" default="yes"/>
</parameter>

<parameter name="arp_mac">
<longdesc lang="en">
MAC address to send the ARP packets too.

You really shouldn't be touching this.

</longdesc>
<shortdesc lang="en">ARP MAC</shortdesc>
<content type="string" default="ffffffffffff"/>
</parameter>

</parameters>

<actions>
<action name="start"   timeout="90" />
<action name="stop"    timeout="100" />
<action name="status" depth="10"  timeout="20s" interval="10s" start-delay="5s" />
<action name="monitor" depth="10"  timeout="20s" interval="10s" start-delay="5s" />
<action name="meta-data"  timeout="5s" />
<action name="validate-all"  timeout="20s" />
</actions>
</resource-agent>
END

	exit $OCF_SUCCESS
}

ip_init() {
	if [ X`uname -s` != "XLinux" ]; then
		ocf_log err "IPaddr2 only supported Linux."
		exit $OCF_ERR_INSTALLED
	fi

	if
          case $__OCF_ACTION in
            start|stop)		ocf_is_root;;
            *)			true;;
          esac
        then
          : YAY!
        else
		ocf_log err "You must be root for $__OCF_ACTION operation."
		exit $OCF_ERR_PERM
	fi
	
	BASEIP="$OCF_RESKEY_ip"
	BRDCAST="$OCF_RESKEY_broadcast"
	NIC="$OCF_RESKEY_nic"
        # Note: We had a version out there for a while which used
        # netmask instead of cidr_netmask. Don't remove this aliasing code!
        if
          [ ! -z "$OCF_RESKEY_netmask" -a -z "$OCF_RESKEY_cidr_netmask" ]
        then
	  OCF_RESKEY_cidr_netmask=$OCF_RESKEY_netmask
	  export OCF_RESKEY_cidr_netmask
        fi
	NETMASK="$OCF_RESKEY_cidr_netmask"
	IFLABEL="$OCF_RESKEY_iflabel"
	IF_MAC="$OCF_RESKEY_mac"

	LVS_SUPPORT=0
	if [ x"${OCF_RESKEY_lvs_support}" = x"true" \
	    -o x"${OCF_RESKEY_lvs_support}" = x"on" \
	    -o x"${OCF_RESKEY_lvs_support}" = x"1" ]; then
	    LVS_SUPPORT=1
	fi

	IP_INC_GLOBAL=${OCF_RESKEY_CRM_meta_clone_max:-1}
	IP_INC_NO=`expr $OCF_RESKEY_CRM_meta_clone + 1`
	IP_CIP_HASH="${OCF_RESKEY_clusterip_hash}"

	if [ $LVS_SUPPORT -gt 0 ] && [ $IP_INC_GLOBAL -gt 1 ]; then
		ocf_log err "LVS and load sharing do not go together well"
		exit OCF_ERR_ARGS
	fi

	ARP_INTERVAL_MS=${OCF_RESKEY_arp_interval:-200}
	ARP_REPEAT=${OCF_RESKEY_arp_count:-5}
	ARP_BACKGROUND=${OCF_RESKEY_arp_bg:-yes}
	ARP_NETMASK=${OCF_RESKEY_arp_mac:-ffffffffffff}

	if ocf_is_decimal "$IP_INC_GLOBAL" && [ $IP_INC_GLOBAL -gt 0 ]; then
		:
	else
		ocf_log err "Invalid OCF_RESKEY_incarnations_max_global [$IP_INC_GLOBAL], should be positive integer"
		exit $OCF_ERR_ARGS
	fi

	  
	# Validation is performed in ip_validate()...
	#
	# $FINDIF now takes its parameters from the environment
	#
	if
	  NICINFO=`$FINDIF -C`
        then
	    NICINFO=`echo $NICINFO | sed -e 's/netmask\ //;s/broadcast\ //'`
	    NIC=`echo "$NICINFO" | cut -d" " -f1`
	    NETMASK=`echo "$NICINFO" | cut -d" " -f2`
	    BRDCAST=`echo "$NICINFO" | cut -d" " -f3`
	else
	    ocf_log err "[$FINDIF -C] failed"
  	    exit $OCF_ERR_ARGS
	fi
	
	SENDARPPIDFILE="$SENDARPPIDDIR/send_arp-$BASEIP"

	case $NIC in
	    *:*)
		IFLABEL=$NIC
		NIC=`echo $NIC | sed 's/:.*//'`
		;;
	    *)
		if [ -n "$IFLABEL" ]; then
			IFLABEL=${NIC}:${IFLABEL}
		fi
		;;
	esac

	IP_CIP=
	
	if [ "$IP_INC_GLOBAL" -gt 1 ]; then
		IP_CIP="yes"
		if [ -z "$IF_MAC" ]; then
			# Choose a MAC
			# 1. Concatenate some input together
			# 2. This doesn't need to be a cryptographically
			#    secure hash.
			# 3. Drop everything after the first 6 octets (12 chars)
			# 4. Delimit the octets with ':'
			# 5. Make sure the first octet is odd,
			#    so the result is a multicast MAC
			IF_MAC=`echo $BASEIP $NETMASK $BRDCAST |	\
				md5sum |				\
				sed -e 's#\(............\).*#\1#'	\
				    -e 's#..#&:#g; s#:$##'		\
				    -e 's#^\(.\)[02468aAcCeE]#\11#'`
		fi
		IP_CIP_FILE="/proc/net/ipt_CLUSTERIP/$BASEIP"
	fi
}

#
#	Find out which interface serves the given IP address
#	The argument is an IP address, and its output
#	is an interface name (e.g., "eth0").
#
find_interface() {
	#
	# List interfaces but exclude FreeS/WAN ipsecN virtual interfaces
	#
	local iface=`$IP2UTIL -o -f inet addr show | grep "\ $BASEIP/" \
		| cut -d ' ' -f2 | grep -v '^ipsec[0-9][0-9]*$'`
	echo $iface
	return 0
}

#
#        Delete an interface
#
delete_interface () {
	ipaddr="$1"
	iface="$2"
	netmask="$3"

	CMD="$IP2UTIL -f inet addr delete $ipaddr/$netmask dev $iface"

	ocf_log info "$CMD"
	$CMD

	if [ $? -ne 0 ]; then
		return $OCF_ERR_GENERIC
	fi

	CMD="$IP2UTIL -o -f inet addr show $iface"

	ocf_log info "$CMD"
	ADDR=`$CMD`

	if [ $? -ne 0 -o ! -z "$ADDR" ]; then
		return $?
	fi

	CMD="$IP2UTIL link set $iface down"

	ocf_log info "$CMD"
	$CMD
	return $?
}

#
#        Add an interface
#
add_interface () {
	ipaddr="$1"
	netmask="$2"
	broadcast="$3"
	iface="$4"
	label="$5"

	CMD="$IP2UTIL -f inet addr add $ipaddr/$netmask brd $broadcast dev $iface"

	if [ ! -z "$label" ]; then
		CMD="$CMD label $label"
	fi

	ocf_log info "$CMD"
	$CMD

	if [ $? -ne 0 ]; then
		return $OCF_ERR_GENERIC
	fi

	CMD="$IP2UTIL link set $iface up"

	ocf_log info "$CMD"
	$CMD

	return $?
}

#
#        Delete a route
#
delete_route () {
	prefix="$1"
	iface="$2"

	CMD="$IP2UTIL route delete $prefix dev $iface"

	ocf_log info "$CMD"
	$CMD

	return $?
}

#      On Linux systems the (hidden) loopback interface may
#      conflict with the requested IP address. If so, this
#      unoriginal code will remove the offending loopback address
#      and save it in VLDIR so it can be added back in later
#      when the IPaddr is released.
#
#      TODO: This is very ugly and should be controlled by an additional
#      instance parameter. Or even: multi-state, with the IP only being
#      "active" on the master!?
#
remove_conflicting_loopback() {
	ipaddr="$1"
	netmask="$2"
	broadcast="$3"
	ifname="$4"

	ocf_log info "Removing conflicting loopback $ifname."
	if [ -d "$VLDIR/" ] || mkdir -p "$VLDIR/"; then
		: Directory $VLDIR now exists
	else
		ocf_log err "Could not create \"$VLDIR/\" conflicting" \
		       " loopback $ifname cannot be restored."
	fi
	if
		echo "$ipaddr $netmask $broadcast $ifname" > "$VLDIR/$ipaddr"
	then
		: Saved loopback information in $VLDIR/$ipaddr
	else
		ocf_log err "Could not save conflicting loopback $ifname." \
		       "it will not be restored."
	fi
	delete_interface "$ipaddr" "$ifname" "$netmask"
	# Forcibly remove the route (if it exists) to the loopback.
	delete_route "$ipaddr" "$ifname"
}       

#
#	On Linux systems the (hidden) loopback interface may
#	need to be restored if it has been taken down previously
#	by remove_conflicting_loopback()
#
restore_loopback() {
	ipaddr="$1"

	if [ -s "$VLDIR/$ipaddr" ]; then
		ifinfo=`cat "$VLDIR/$ipaddr"`
		ocf_log info "Restoring loopback IP Address " \
		    "$ifinfo."
		add_interface $ifinfo
		rm -f "$VLDIR/$ipaddr"
	fi
}

#
# Run send_arp to note peers about new mac address
#
run_send_arp() {
	ARGS="-i $ARP_INTERVAL_MS -r $ARP_REPEAT -p $SENDARPPIDFILE $NIC $BASEIP auto not_used not_used"
	if [ "x$IP_CIP" = "xyes" ] ; then
	    if [ x = "x$IF_MAC" ] ; then
		MY_MAC=auto
	    else
		MY_MAC=`echo ${IF_MAC} | sed -e 's/://'`
	    fi
	    ARGS="-i $ARP_INTERVAL_MS -r $ARP_REPEAT -p $SENDARPPIDFILE $NIC $BASEIP $MY_MAC not_used not_used"
	fi
	ocf_log info "$SENDARP $ARGS"
	case $ARP_BACKGROUND in
	yes) 
		($SENDARP $ARGS || ocf_log err "Could not send gratuitous arps" &) >&2
		;;
	*)
		$SENDARP $ARGS || ocf_log err "Could not send gratuitous arps"
		;;
	esac
}

# Do we already serve this IP address?
#
# returns:
# ok = served (for CIP: + hash bucket)
# partial = served and no hash bucket (CIP only)
# no = nothing
#
ip_served() {
	cur_nic="`find_interface $BASEIP`"

	if [ -z "$cur_nic" ]; then
		echo "no"
		return 0
	fi

	if [ -z "$IP_CIP" ]; then
		case $cur_nic in
		lo*)	if [ "$LVS_SUPPORT" = "1" ]; then
				echo "no"
				return 0
			fi
			;;
		esac

		echo "ok"
		return 0
	fi

	# Special handling for the CIP:
	if grep -q "^${IP_INC_NO},\|,${IP_INC_NO},\|,${IP_INC_NO}$\|^${IP_INC_NO}$" $IP_CIP_FILE ; then
		echo "ok"
		return 0
	else
		echo "partial"
		return 0
	fi

	exit $OCF_ERR_GENERIC
}

#######################################################################

ip_usage() {
	cat <<END
usage: $0 {start|stop|status|monitor|validate-all|meta-data}

Expects to have a fully populated OCF RA-compliant environment set.
END
}

ip_start() {
	if [ -n "$IP_CIP" ]; then
	    # Cluster IPs need special processing when the first bucket
	    #  is added to the node... take a lock to make sure only one
	    #  process executes that code
	    ocf_take_lock $CIP_lockfile
	    ocf_release_lock_on_exit $CIP_lockfile
	fi

	ip_init

	#
	#	Do we already service this IP address?
	#
	local ip_status=`ip_served`

	if [ "$ip_status" = "ok" ]; then
		exit $OCF_SUCCESS
	fi
	
	if [ -n "$IP_CIP" ] && [ $ip_status = "no" ]; then
		$MODPROBE ip_conntrack
		$IPTABLES -I INPUT -d $BASEIP -i $NIC -j CLUSTERIP \
				--new \
				--clustermac $IF_MAC \
				--total-nodes $IP_INC_GLOBAL \
				--local-node $IP_INC_NO \
				--hashmode $IP_CIP_HASH
		if [ $? -ne 0 ]; then
			ocf_log err "iptables failed"
			exit $OCF_ERR_GENERIC
		fi
	fi

	if [ -n "$IP_CIP" ] && [ $ip_status = "partial" ]; then
		echo "+$IP_INC_NO" >$IP_CIP_FILE
	fi
	
	if [ "$ip_status" = "no" ]; then
		if [ "$LVS_SUPPORT" = "1" ]; then
			case `find_interface $BASEIP` in
			lo*)
				remove_conflicting_loopback $BASEIP 32 255.255.255.255 lo
				;;
			esac
		fi
		
		add_interface $BASEIP $NETMASK $BRDCAST $NIC $IFLABEL
		
		if [ $? -ne 0 ]; then
			ocf_log err "$CMD failed."
			exit $OCF_ERR_GENERIC
		fi
	fi

	case $NIC in
	lo*)
		: no need to run send_arp on loopback
		;;
	*)
		run_send_arp
		;;
	esac
	exit $OCF_SUCCESS
}

ip_stop() {
	ip_init
	local ip_del_if="yes"
	if [ -n "$IP_CIP" ]; then
	    # Cluster IPs need special processing when the last bucket
	    #  is removed from the node... take a lock to make sure only one
	    #  process executes that code
	    ocf_take_lock $CIP_lockfile
	    ocf_release_lock_on_exit $CIP_lockfile
	fi
	
	if [ -f "$SENDARPPIDFILE" ] ; then
		kill `cat "$SENDARPPIDFILE"`
		if [ $? -ne 0 ]; then
			ocf_log warn "Could not kill previously running send_arp for $BASEIP"
		else
			ocf_log info "killed previously running send_arp for $BASEIP"
			rm -f "$SENDARPPIDFILE"
		fi
	fi
	local ip_status=`ip_served`

	if [ $ip_status = "no" ]; then
		: Requested interface not in use
		exit $OCF_SUCCESS
	fi

	if [ -n "$IP_CIP" ]; then
		if [ $ip_status = "partial" ]; then
			exit $OCF_SUCCESS
		fi
		echo "-$IP_INC_NO" >$IP_CIP_FILE
		if [ "x$(cat $IP_CIP_FILE)" = "x" ]; then
			ocf_log info $BASEIP, $IP_CIP_HASH
			i=1
			while [ $i -le $IP_INC_GLOBAL ]; do
				ocf_log info $i
				$IPTABLES -D INPUT -d $BASEIP -i $NIC -j CLUSTERIP \
					--new \
					--clustermac $IF_MAC \
					--total-nodes $IP_INC_GLOBAL \
					--local-node $i \
					--hashmode $IP_CIP_HASH
				i=`expr $i + 1`
			done
		else
			ip_del_if="no"		
		fi
	fi
	
	if [ "$ip_del_if" = "yes" ]; then
		delete_interface $BASEIP $NIC $NETMASK
		if [ $? -ne 0 ]; then
			exit $OCF_ERR_GENERIC
		fi
	
		if [ "$LVS_SUPPORT" = 1 ]; then
			restore_loopback "$BASEIP"
		fi
	fi

	exit $OCF_SUCCESS
}

ip_monitor() {
	ip_init
	# TODO: Implement more elaborate monitoring like checking for
	# interface health maybe via a daemon like FailSafe etc...

	local ip_status=`ip_served`
	case $ip_status in
	ok)
		return $OCF_SUCCESS
		;;
	partial|no)
		exit $OCF_NOT_RUNNING
		;;
	*)
		# Errors on this interface?
		return $OCF_ERR_GENERIC
		;;
	esac
}

ip_validate() {
    check_binary $IP2UTIL
    if [ -n "$IP_CIP" ]; then
	check_binary $IPTABLES
	check_binary $MODPROBE
    fi

    ip_init

# $BASEIP, $NETMASK, $NIC , $IP_INC_GLOBAL, and $BRDCAST have been checked within ip_init,
# do not bother here.
	
    if ocf_is_decimal "$ARP_INTERVAL_MS" && [ $ARP_INTERVAL_MS -gt 0 ]; then
	:
    else
	ocf_log err "Invalid OCF_RESKEY_arp_interval [$ARP_INTERVAL_MS]"
	exit $OCF_ERR_ARGS
    fi

    if ocf_is_decimal "$ARP_REPEAT" && [ $ARP_REPEAT -gt 0 ]; then
	:
    else
	ocf_log err "Invalid OCF_RESKEY_arp_count [$ARP_REPEAT]"
	exit $OCF_ERR_ARGS
    fi

    if [ -n "$IP_CIP" ]; then

	local valid=1

	case $IP_CIP_HASH in
	sourceip|sourceip-sourceport|sourceip-sourceport-destport)
		;;
	*)
		ocf_log err "Invalid OCF_RESKEY_clusterip_hash [$IP_CIP_HASH]"
		exit $OCF_ERR_ARGS
		;;
	esac

	if [ "$LVS_SUPPORT" = 1 ]; then
		ecf_log err "LVS and load sharing not advised to try"
		exit $OCF_ERR_ARGS
	fi

	case $IF_MAC in
	[0-9a-zA-Z][1379bBdDfF][^0-9a-zA-Z][0-9a-zA-Z][0-9a-zA-Z][^0-9a-zA-Z][0-9a-zA-Z][0-9a-zA-Z][^0-9a-zA-Z][0-9a-zA-Z][0-9a-zA-Z][^0-9a-zA-Z][0-9a-zA-Z][0-9a-zA-Z][^0-9a-zA-Z][0-9a-zA-Z][0-9a-zA-Z])
		;;
	*)
		valid=0
		;;
	esac

	if [ $valid -eq 0 ]; then
	  ocf_log err "Invalid IF_MAC [$IF_MAC]"
	  exit $OCF_ERR_ARGS
	fi

    fi

	exit $OCF_SUCCESS
}

case $__OCF_ACTION in
meta-data)	meta_data
		;;
start)		ip_start
		;;
stop)		ip_stop
		;;
status)		ip_init
		ip_status=`ip_served`
		if [ $ip_status = "ok" ]; then
			echo "running"
			exit $OCF_SUCCESS
		else
			echo "stopped"
			exit $OCF_NOT_RUNNING
		fi
		;;
monitor)	ip_monitor
		;;
validate-all)	ip_validate
		;;
usage|help)	ip_usage
		exit $OCF_SUCCESS
		;;
*)		ip_usage
		exit $OCF_ERR_UNIMPLEMENTED
		;;
esac
