flow:
  - start|DEFAULT_ROUTE:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|ROUTE_NET_INFO:
  - return|ROUTE_NET_INFO:
  - start|ROUTE_CHECK_TEL_URI:
  - return|ROUTE_CHECK_TEL_URI:
  - start|ROUTE_PRX_REQUEST:
  - start|ROUTE_INITVARS:
  - return|ROUTE_INITVARS:
  - start|ROUTE_LOCAL:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - exit|ROUTE_EXIT:
sip_in:
  - 'CANCEL sip:439333111@127.2.0.1:\d+ SIP/2.0'
  - 'To: <sip:439333111@spce.test>'
  - 'From: <sip:4311002@spce.test>;tag=[\w-]+'
  - 'CSeq: \d+ CANCEL'
  - 'Contact: <sip:127.0.0.1:508[08];transport=udp>'
  - 'P-LB-Uptime: \d+'
  - 'P-Caller-UUID: [% spce_test.testuser1002.uuid %]'
  - 'P-NGCP-Caller-Info: <sip:testuser1002@spce.test>;ip=127.126.0.1;port=\d+;primary=4311002'
  - 'P-NGCP-Callee-Info: <sip:43110021003@spce.test>;ip=127.0.0.1;port=5060;primary=43110021003'
  - 'P-Asserted-Identity: <sip:4311002@spce.test>'
  - 'P-D-Uri: sip:lb@127.0.0.1;lr;socket=sip:127.0.0.1:5060'
  - 'Content-Length: 0'
sip_out:
  - [
      'SIP/2.0 100 Trying',
      'To: <sip:439333111@spce.test>',
      'From: <sip:4311002@spce.test>;tag=[\w-]+',
      'CSeq: \d+ CANCEL',
      'Server: Sipwise NGCP Proxy',
      'Content-Length: 0',
    ]
  - [
      'CANCEL sip:439333111@127.2.0.1:\d+ SIP/2.0',
      'From: <sip:4311002@spce.test>;tag=[\w-]+',
      'To: <sip:439333111@spce.test>',
      'CSeq: \d+ CANCEL',
      'Content-Length: 0',
    ]
  - [
      'SIP/2.0 200 canceling',
      'To: <sip:439333111@spce.test>;tag=[\w-]+',
      'From: <sip:4311002@spce.test>;tag=[\w-]+',
      'CSeq: \d+ CANCEL',
      'Server: Sipwise NGCP Proxy',
      'Content-Length: 0',
    ]
