flow:
  - start|DEFAULT_ONREPLY:
  - start|REPLY_ROUTE_NAT:
      $avp(lua_dlg_profile): [
        "local",
        "total"
      ]
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|ROUTE_APPLY_HEADER_RULES:
  - return|ROUTE_APPLY_HEADER_RULES:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|REPLY_ROUTE_NAT_CONTINUE:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - exit|ROUTE_EXIT:
sip_in:
  - '^SIP/2.0 180 Ringing'
  - 'CSeq: \d+ INVITE'
sip_out:
  - [
      '^SIP/2.0 180 Ringing',
      'CSeq: \d+ INVITE',
    ]
