flow:
  - start|DEFAULT_ONREPLY:
  - start|REPLY_ROUTE_NAT:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|ROUTE_APPLY_HEADER_RULES:
  - return|ROUTE_APPLY_HEADER_RULES:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|REPLY_ROUTE_NAT_CONTINUE:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - exit|ROUTE_EXIT:
sip_in:
  - '^SIP/2.0 200 OK'
  - 'From: <sip:[% invite_redirect_tel_uri_scenarios_test.testuser1000.phone_number %]@invite-redirect-tel-uri.scenarios.test>;tag=[\w-]+'
  - 'To: <sip:\+[% invite_redirect_tel_uri_scenarios_test.testuser1001.phone_number %]@invite-redirect-tel-uri.scenarios.test'
  - 'CSeq: \d+ BYE'
  - 'Content-Length: 0'
sip_out:
  - [
      '^SIP/2.0 200 OK',
      'From: <tel:\+[% invite_redirect_tel_uri_scenarios_test.testuser1000.phone_number %]>;tag=[\w-]+',
      'To: <tel:\+[% invite_redirect_tel_uri_scenarios_test.testuser1001.phone_number %]>;tag=[\w-]+',
      'CSeq: \d+ BYE',
      'Content-Length: 0'
    ]
