flow:
  - start|DEFAULT_ONREPLY:
  - start|REPLY_ROUTE_NAT:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|ROUTE_APPLY_HEADER_RULES:
  - return|ROUTE_APPLY_HEADER_RULES:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|REPLY_ROUTE_NAT_CONTINUE:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - exit|ROUTE_EXIT:
sip_in:
  - '^SIP/2.0 200 OK'
  - 'CSeq: 3 BYE'
  - 'Content-Length: 0'
  - 'From: <sip:[% invite_blockout_pinoverride_scenarios_test.testuser1002.phone_number %]@'
  - 'To: <sip:\*80\*444[% invite_blockout_pinoverride_scenarios_test.testuser1003.phone_number %]@'
sip_out:
  - [
      '^SIP/2.0 200 OK',
      'CSeq: 3 BYE',
      'Content-Length: 0',
      'From: <sip:testuser1002@',
      'To: <sip:\*80\*444[% invite_blockout_pinoverride_scenarios_test.testuser1003.phone_number %]@'
    ]
