flow:
  - start|DEFAULT_ONREPLY:
  - start|REPLY_ROUTE_NAT:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|ROUTE_APPLY_HEADER_RULES:
  - return|ROUTE_APPLY_HEADER_RULES:
  - start|REPLY_SCA_UPDATE:
  - return|REPLY_SCA_UPDATE:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|ROUTE_FIX_PBX_STOP_RECORDS:
  - return|ROUTE_FIX_PBX_STOP_RECORDS:
  - start|REPLY_ROUTE_RTPENGINE:
  - return|REPLY_ROUTE_RTPENGINE:
  - start|REPLY_ROUTE_NAT_CONTINUE:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - start|dialog:start:
  - return|dialog:start:
  - return|dialog:start:
sip_in:
  - '^SIP/2.0 200 OK'
  - 'From: <sip:testuser1002'
  - 'To: <sip:1003@'
  - 'CSeq: \d+ INVITE'
  - 'Content-Type: application/sdp'
sip_out:
  - [
      '^SIP/2.0 200 OK',
      'CSeq: \d+ INVITE',
      'From: <sip:testuser1002@',
      'To: <sip:1003@',
      'Content-Type: application/sdp',
    ]
