flow:
  - start|REPLY_ROUTE_NAT:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|REPLY_SCA_UPDATE:
  - return|REPLY_SCA_UPDATE:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - exit|ROUTE_EXIT:
sip_in:
  - '^SIP/2.0 180 Ringing'
  - 'From: <sip:testuser1003@spce.test>;tag='
  - 'To: <sip:1002@spce.test>;tag='
  - 'CSeq: 2 INVITE'
  - 'Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE'
  - 'Call-Info: <sip:spce\.test>;appearance-index=1'
  - 'Contact: <sip:127.0.0.1:5085;transport=udp>'
  - 'Content-Length: 0'
sip_out:
  - [
      '^SIP/2.0 180 Ringing',
      'From: <sip:testuser1003@spce.test>;tag=',
      'To: <sip:1002@spce.test>;tag=',
      'CSeq: 2 INVITE',
      'Allow: INVITE, INFO, PRACK, ACK, BYE, CANCEL, OPTIONS, NOTIFY, REGISTER, SUBSCRIBE, REFER, PUBLISH, UPDATE, MESSAGE',
      'Contact: <sip:127.0.0.1:5085;transport=udp>',
      'Content-Length: 0',
      'P-COLP-Identity: \"1002\" <sip:1002@spce.test>',
      'P-Out-Socket: udp:127.0.0.1:5060',
    ]
