flow:
  - start|REPLY_ROUTE_NAT:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|REPLY_SCA_UPDATE:
  - return|REPLY_SCA_UPDATE:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|REPLY_ROUTE_RTPENGINE:
  - return|REPLY_ROUTE_RTPENGINE:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - start|dialog:start:
  - return|dialog:start:
  - return|dialog:start:
sip_in:
  - '^SIP/2.0 200 OK'
  - 'From: <sip:testuser1003@spce.test>;tag='
  - 'To: <sip:1002@spce.test>;tag='
  - 'CSeq: 2 INVITE'
  - 'Call-Info: <sip:spce\.test>;appearance-index=1'
  - 'Contact: <sip:127.0.0.1:5085;transport=udp>'
  - 'Content-Type: application/sdp'
  - 'Content-Length: \d+'
sip_out:
  - [
      '^SIP/2.0 200 OK',
      'From: <sip:testuser1003@spce.test>;tag=',
      'To: <sip:1002@spce.test>;tag=',
      'CSeq: 2 INVITE',
      'Contact: <sip:127.0.0.1:5085;transport=udp>',
      'Content-Type: application/sdp',
      'Content-Length: \d+',
      'P-COLP-Identity: \"1002\" <sip:1002@spce.test>',
      'P-Out-Socket: udp:127.0.0.1:5060',
    ]
