flow:
  - start|DEFAULT_ONREPLY:
  - start|REPLY_ROUTE_NAT:
  - start|ROUTE_ENTRY:
  - return|ROUTE_ENTRY:
  - start|ROUTE_APPLY_HEADER_RULES:
  - return|ROUTE_APPLY_HEADER_RULES:
  - start|ROUTE_PREPARE_UA:
  - return|ROUTE_PREPARE_UA:
  - start|REPLY_ROUTE_NAT_CONTINUE:
  - start|ROUTE_EXIT:
  - start|ROUTE_RUNTIME:
  - return|ROUTE_RUNTIME:
  - exit|ROUTE_EXIT:
sip_in:
  - '^SIP/2.0 200 OK'
  - 'From: <sip:\*55\*1420@reminder.scenarios.test>;tag='
  - 'To: <sip:[% scenarios.0.username %]@reminder.scenarios.test>;tag='
  - 'CSeq: \d+ BYE'
  - 'Content-Length:\s+0'
  - 'P-NGCP-Src-Ip: [% scenarios.0.ip %]'
  - 'P-NGCP-Src-Port: [% scenarios.0.port %]'
  - 'P-NGCP-Src-Proto: udp'
  - 'P-NGCP-Src-Af: 4'
sip_out:
  - [
       '^SIP/2.0 200 OK',
       'CSeq: \d+ BYE'
    ]
