topoh Module

Daniel-Constantin Mierla

   <miconda@gmail.com>

Edited by

Daniel-Constantin Mierla

   <miconda@gmail.com>

   Copyright © 2009 FhG FOKUS
     __________________________________________________________________

   Table of Contents

   1. Admin Guide

        1. Overview
        2. Dependencies

              2.1. Kamailio Modules
              2.2. External Libraries or Applications

        3. Parameters

              3.1. mask_key (str)
              3.2. mask_ip (str)
              3.3. mask_callid (integer)
              3.4. uparam_name (str)
              3.5. uparam_prefix (str)
              3.6. vparam_name (str)
              3.7. vparam_prefix (str)
              3.8. callid_prefix (str)
              3.9. sanity_checks (integer)

        4. Functions

              4.1.

   List of Examples

   1.1. Set mask_key parameter
   1.2. Set mask_ip parameter
   1.3. Set mask_callid parameter
   1.4. Set uparam_name parameter
   1.5. Set uparam_prefix parameter
   1.6. Set vparam_name parameter
   1.7. Set vparam_prefix parameter
   1.8. Set callid_prefix parameter
   1.9. Set sanity_checks parameter

Chapter 1. Admin Guide

   Table of Contents

   1. Overview
   2. Dependencies

        2.1. Kamailio Modules
        2.2. External Libraries or Applications

   3. Parameters

        3.1. mask_key (str)
        3.2. mask_ip (str)
        3.3. mask_callid (integer)
        3.4. uparam_name (str)
        3.5. uparam_prefix (str)
        3.6. vparam_name (str)
        3.7. vparam_prefix (str)
        3.8. callid_prefix (str)
        3.9. sanity_checks (integer)

   4. Functions

        4.1.

1. Overview

   This module hides the SIP routing headers that show topology details.
   It it is not affected by the server being transaction stateless or
   stateful. The script interpreter gets the SIP messages decoded, so all
   existing functionality is preserved.

   The module is transparent for the configuration writer. It only needs
   to be loaded (tune the parameters if needed). The SIP server can be
   restarted whitout affecting ongoing calls - once it is up, can
   encode/decode topology details, thus no call will be lost.

   By using same mask_key, many SIP servers can decode the message, for
   example, applicable for servers behind load balancers.

2. Dependencies

   2.1. Kamailio Modules
   2.2. External Libraries or Applications

2.1. Kamailio Modules

   The following modules must be loaded before this module:
     * rr module - server must perform record routing to ensure in-dialog
       requests are encoded/decoded.

2.2. External Libraries or Applications

   The following libraries or applications must be installed before
   running Kamailio with this module loaded:
     * None. In the future the module can be enhanced to use a stronger
       encryption algorithm.

3. Parameters

   3.1. mask_key (str)
   3.2. mask_ip (str)
   3.3. mask_callid (integer)
   3.4. uparam_name (str)
   3.5. uparam_prefix (str)
   3.6. vparam_name (str)
   3.7. vparam_prefix (str)
   3.8. callid_prefix (str)
   3.9. sanity_checks (integer)

3.1. mask_key (str)

   Keyword to mask the headers.

   Default value is "_static_value_".

   Example 1.1. Set mask_key parameter
...
modparam("topoh", "mask_key", "some secret here")
...

3.2. mask_ip (str)

   IP address to be used in masked headers to build valid SIP URIs. Can be
   any IP address, even a private-space IP address (e.g., 192.168.1.1),
   but must not be SIP server's local IP address. It is not used at all
   for SIP routing.

   Default value is "10.1.1.10".

   Example 1.2. Set mask_ip parameter
...
modparam("topoh", "mask_ip", "192.168.0.1")
...

3.3. mask_callid (integer)

   Whether to encode the Call-id: header. Some SIP extensions include the
   Call-id in the SIP message payload or header, so it is safe to not
   encode Call-id in such cases. Well-known extensions such as call
   transfer or conference join will be added to work with encoded Call-id.

   Default value is 0 (do not mask).

   Example 1.3. Set mask_callid parameter
...
modparam("topoh", "mask_callid", 1)
...

3.4. uparam_name (str)

   Name of URI parameter where to store encoded value.

   Default value is "line".

   Example 1.4. Set uparam_name parameter
...
modparam("topoh", "uparam_name", "myparam")
...

3.5. uparam_prefix (str)

   Prefix to be added in encoded URI parameters.

   Default value is "sr-".

   Example 1.5. Set uparam_prefix parameter
...
modparam("topoh", "uparam_prefix", "xyz")
...

3.6. vparam_name (str)

   Name of Via: parameter used to store encoded value.

   Default value is "branch".

   Example 1.6. Set vparam_name parameter
...
modparam("topoh", "vparam_name", "myv")
...

3.7. vparam_prefix (str)

   Prefix to be added in encoded Via: parameters.

   Default value is "z9hG4bKsr-".

   Example 1.7. Set vparam_prefix parameter
...
modparam("topoh", "vparam_prefix", "xyz")
...

3.8. callid_prefix (str)

   Prefix to be added in encoded Call-ID: headers.

   Default value is "!!:".

   Example 1.8. Set callid_prefix parameter
...
modparam("topoh", "callid_prefix", "***")
...

3.9. sanity_checks (integer)

   If set to 1, topoh module will bind to sanity module in order to
   perform sanity checks over received SIP request. Default sanity checks
   are done. It is useful to check if received request is well formated
   before proceeding to encoding/decoding.

   Default value is 0 (do not bind to sanity module).

   Example 1.9. Set sanity_checks parameter
...
modparam("topoh", "sanity_checks", 1)
...

4. Functions

   4.1.

   None.
