# SIP / UDP
listen=udp:11.22.33.44:6060
# SIP / TCP
#listen=tcp:11.22.33.44:6060
# SIP / TCP/TLS
#listen=tls:11.22.33.44:6061

#!define NETWORKNAME "ims.mnc001.mcc001.3gppnetwork.org"
#!define HOSTNAME "scscf.mnc001.mcc001.3gppnetwork.org"
#!define URI "sip:scscf.mnc001.mcc001.3gppnetwork.org:6060"

alias=scscf.mnc001.mcc001.3gppnetwork.org

# ENUM-Server to query:
#!define ENUM_SUFFIX "mnc001.mcc001.3gppnetwork.org."

# SIP-Address of capturing node, if not set, capturing is disabled.
##!define CAPTURE_NODE "sip:127.0.0.1:9060"

# Connection URL for the database:
# For use with a single database:
##!define DB_URL "mysql://scscf:heslo@127.0.0.1/scscf"

# For use with DB_Cluster: con1 (primary), con2 (backup)
##!define DB_URL "con1=>mysql://scscf:heslo@127.0.0.1/scscf"
##!define DB_URL2 "con2=>mysql://scscf:heslo@127.0.0.1/scscf"

# Select Authorization Algorhithm:
##!define REG_AUTH_DEFAULT_ALG "AKAv1-MD5"
##!define REG_AUTH_DEFAULT_ALG "AKAv2-MD5"
##!define REG_AUTH_DEFAULT_ALG "MD5"
##!define REG_AUTH_DEFAULT_ALG "CableLabs-Digest"
##!define REG_AUTH_DEFAULT_ALG "3GPP-Digest"
##!define REG_AUTH_DEFAULT_ALG "TISPAN-HTTP_DIGEST_MD5"
# Let the HSS decide
#!define REG_AUTH_DEFAULT_ALG "HSS-Selected"

# Number of TCP Processes
#!define TCP_PROCESSES 3

##!define RO_FORCED_PEER "32260@3gpp.org"
#!define RO_DESTINATION "hssocs.voiceblue.com"
#!define RO_ROOT "32260@3gpp.org"
#!define RO_EXT "ext"
#!define RO_MNC "07"
#!define RO_MCC "262"
#(see https://en.wikipedia.org/wiki/Mobile_country_code_(MCC))
#!define RO_RELEASE "8"
# See http://tools.ietf.org/html/rfc4006#section-4.1.2 for the definition of the Service-Context

##!define XMLRPC_WHITELIST_1 "127.0.0.1"
##!define XMLRPC_WHITELIST_2 "127.0.0.1"
##!define XMLRPC_WHITELIST_3 "127.0.0.1"

# Several features can be enabled using '#!define WITH_FEATURE' directives:
#
# *** To run in debug mode: 
#     - define WITH_DEBUG
#
# *** To enable TCP support execute:
#     - define WITH_TCP
#
# *** To enable XMLRPC support execute:
#     - define WITH_XMLRPC
#     - this will automagically enable TCP
#
# *** To enable the Ro-Interface:
#     - Configure Ro-Diameter-Interface in scscf.xml
#     - define WITH_RO
#
# *** To enable a Homer SIP-Capter-Node:
#     - define CAPTURE_NODE with a proper address
#
# Enabled Features for this host:
##!define WITH_DEBUG
##!define WITH_XMLRPC
##!define WITH_RO
##!define WITH_RO_TERM
##!define WITH_AUTH
