# Hello Strapdown

    #sip_profile_collection

    This is a child of `profile_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_objectName_` | _objectName_ | `SIP Profiles` |
    `_position_` | _position_ |  |

    #cg_network_element

    This is a child of `channel_group`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `CGId` | CGId |  |
    `IPType` | IPType |  |
    `MinDigits` | Minimum # of Digits | `Not Used` | `Not Used`, `int_range(1,24)`
    `_cachedNotify_` | Cached Notify | `ChannelGroups` |
    `ElementType` | ElementType |  |
    `TotalSamTimeout` | Total Overlap Timeout |  |
    `InterSamTimeout` | Inter SAM Timeout |  |
    `GWId` | GWId |  |
    `_position_` | _position_ |  |
    `Name` | IP Network Element |  |
    `ElementTypeInt` | ElementTypeInt | `2` |
    `ResourceGroupIdCounter` | ResourceGroupIdCounter | `0x01` |
    `_objectName_` | _objectName_ |  |
    `AddressType` | AddressType |  |
    `OverlapEnable` | Overlap Enable | `Not Used` | `Not Used`, `Disabled`, `Enabled`
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `SGPId` | SGPId |  |

    #external_gateway_collection

    This is a child of `external_network_elements`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_position_` | _position_ |  |
    `_objectName_` | _objectName_ | `External Gateways` |

    #packet_facility_collection

    This is a child of `facility`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `NodeNetworkMultimedia` | Network Multimedia Total |  |
    `PacketMultimedia` | Packet Multimedia Available | `0` |
    `NextRTPPortMedia0` | Next RTP Port Media 0 | `0` |
    `NetworkMultimedia` | Network Multimedia Available | `0` |
    `NextRTPPortMedia1` | Next RTP Port Media 1 | `0` |
    `PacketAudio` | Packet Audio Available | `0` |
    `NextSpanID` | Next Span ID | `8192` |
    `_position_` | _position_ |  |
    `NodePacketAudio` | Packet Audio Total |  |
    `_objectName_` | _objectName_ | `Packet Facilities` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `NodePacketMultimedia` | Packet Multimedia Total |  |

    #sip_profile

    This is a child of `sip_profile_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `Precondition` | Precondition Support | `Disabled` | `Disabled`, `Required`, `Required and Relay`, `Relay`
    `CodecPriority` | Codec Priority | `Local` | `Local`, `Remote`
    `RetryCount` | INVITE Retransmission Attempts | `Retransmit All` | `Retransmit All`, `int_range(1,5)`
    `Privacy` | Privacy | `Disabled` | `Disabled`, `P-Asserted only`, `Remote-Party only`, `Both`
    `SRTPMode` | SRTP Mode | `Disabled` | `Disabled`, `Mandatory`, `RTP fallback`
    `_position_` | _position_ |  |
    `LoopDetectionURI` | Loop Detection Method | `To Header` | `To Header`, `R-URI`
    `Trusted` | Trusted | `Enabled` | `Disabled`, `Enabled`
    `RingingBehavior` | 180 Ringing Behavior | `Send 183 Progress w/SDP` | `Send 183 Progress w/SDP`, `Send 180 Ringing`
    `OutboundDelayedMedia` | Outbound Delayed Media | `Disabled` | `Disabled`, `Enabled`
    `LoopDetection` | Loop Detection | `Enabled` | `Enabled`, `Disabled`, `Disabled with No Header Check`
    `AllowSameIPRedirection` | Redirection To Same IP/Port | `Disallow` | `Disallow`, `Allow`
    `RedirectSupport` | 3XX Redirect Support | `Enabled` | `Disabled`, `Enabled`
    `ProfileId` | ID | `0` |
    `IDName` | IDName | `ID: 0 - SIP Default` |
    `PrackSupport` | PRACK Support | `Disabled` | `Disabled`, `Supported`, `Required`
    `ProfileName` | Name | `SIP Default` |
    `PAID_RPID_DisplayNameBehavior` | PAID RPID Display Name | `When none received send user part of URI` | `When none received send user part of URI`, `When none received send none`
    `InfoKeepAliveSupport` | INFO Keep-Alive Support | `Disabled` | `Disabled`, `Enabled`
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_objectName_` | _objectName_ | `SIP Profile: SIP Default` |
    `PrackTimer` | PRACK Timer (s) | `150` | `60`, `150`
    `TLV_SIPSGP` | SIP TAG |  |

    #ip_profile

    This is a child of `ip_profile_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `TunnelingEnable` | H245 Outbound Tunneling | `Enable` | `Enable`, `Disable`
    `MediaPayloadSize` | Descendant Media Payload Size |  |
    `MediaStreamInfo` | Media Stream Info |  |
    `VoipParamSet` | VoIP Parameter Settings |  |
    `Name` | Name | `IP_Profile_1` |
    `RelayPayloadType16000` | Digit Relay Packet Type (16000) | `102` | `int_range(96,100)`, `int_range(102,127)`
    `TosSettings` | Descendant TOS Settings |  |
    `SilenceSupression` | Silence Supression | `Disable` | `Disable`, `Enable`
    `MediaPayloadDesc` | Descendant Media Payload Description |  |
    `MediaPayloadMinSize` | Descendant Media Payload Size |  |
    `RTPPayloadType` | RTP Payload Type for Redundancy | `Not Used` |
    `SourcePortValidate` | Source Port Validate | `Enable` | `Disable`, `Enable`
    `_objectName_` | _objectName_ | `IP Profile: IP_Profile_1` |
    `MediaCodecInfo` | Media Codec Info |  |
    `HighJitter` | High Jitter | `Disable` | `Disable`, `Enable`
    `FaxBypassCodec` | Fax Bypass Codec | `G711 ulaw` | `G711 ulaw`, `G711 alaw`
    `MediaInactivityMode` | Media Inactivity Timer | `Disable` | `Disable`, `Enable`
    `FaxMode` | Fax Mode | `Enable Bypass` | `Disable`, `Enable Relay (T.38)`, `Enable Bypass`, `Relay Fallback to Bypass`
    `InitialInactivity` | Initial Media Inactivity Timer Value | `181` |
    `MediaPayloadMaxSize` | Descendant Media Payload Max Size |  |
    `ModemMode` | Modem Behavior | `Bypass` | `Bypass`, `Disabled`
    `RelayPayloadType` | Digit Relay Packet Type | `101` | `int_range(96,101)`, `int_range(103,127)`
    `_position_` | _position_ |  |
    `DigitRelay` | Digit Relay | `DTMF In-band` | `DTMF In-band`, `DTMF Packetized`, `DTMF via Signaling`
    `MediaType` | Media Type | `Disable` | `Disable`, `Enable`
    `MediaPayloadType` | Descendant Media Payload Type |  |
    `_cachedNotify_` | Cached Notify | `Profiles` |
    `FaxPacketRedundancy` | Fax Packet Redundancy | `No Redundancy` | `No Redundancy`, `Redundancy Level 1`, `Redundancy Level 2`, `Redundancy Level 3`
    `ID` | ID | `1` |
    `RTPRedundancy` | RTP Redundancy | `No Redundancy` | `No Redundancy`, `Redundancy Level 1`
    `InitialInactivityMode` | Initial Media Inactivity Timer | `Disable` | `Disable`, `Enable`
    `MediaInactivity` | Media Inactivity Timer Value | `30` |
    `EchoCancel` | Echo Cancellation | `Enabled (NLP Enabled)` | `Enabled (NLP Enabled)`, `Enabled (NLP Disabled)`, `Disabled`

    #route_element

    This is a child of `route_table`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------

    #network

    This is a child of `bn2020`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_objectName_` | _objectName_ | `IP Network` |
    `_position_` | _position_ |  |
    `IPFirewall` | IP Firewall | `Enable` | `Disable`, `Enable`
    `ConfigTableID` | Cfg Table Id | `0x0022` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |

    #profile_collection

    This is a child of `root`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_cached_` | Cached |  |
    `_objectName_` | _objectName_ | `Profiles` |
    `_position_` | _position_ |  |
    `IPProfileTableName` | IPProfile Tables | `IPProfile Tables` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |

    #ip_profile_collection

    This is a child of `profile_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_position_` | _position_ |  |
    `_objectName_` | _objectName_ | `IP Profiles` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |

    #routing_configuration

    This is a child of `root`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_objectName_` | _objectName_ | `Routing Configuration` |
    `_position_` | _position_ |  |
    `Profile0` | Profile 0 | `Default Profile PSTN` |
    `Profile1` | Profile 1 | `Default Profile Subscriber` |

    #route_table

    This is a child of `route_table_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------

    #vocoder_profile

    This is a child of `ip_profile`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `MinPayloadSize` | Minimum Payload Size (ms) | `10` | `10`, `20`, `30`
    `AnnexBIngress` | Annex B Ingress | `Disabled` | `Disabled`, `Reject Call, if Different`, `Echo Recieved`, `Send Configured`
    `OctetAlign` | Octet Align | `1` |
    `PayloadType` | Payload Type | `G711 ulaw` | `AMR`, `AMR Bandwidth Efficient`, `AMR-WB`, `AMR-WB Bandwidth Efficient`, `Clear Channel`, `G711 alaw`, `G711 ulaw`, `G723 5.3 Kbps`, `G723 6.3 Kbps`, `G729`, `G722`, `iLBC 20ms`, `iLBC 30ms`, `GSM-FR Static Payload Type`, `GSM-FR Dynamic Payload Type`, `G726-32/G721 Static Payload Type`, `G726-32/G721 Dynamic Payload Type`, `GSM-EFR`
    `_objectName_` | _objectName_ | `Vocoder Profile: G711 ulaw` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `PayloadSize` | Preferred Payload Size (ms) | `20` | `10`, `20`, `30`
    `AnnexBSupport` | Annex B Support | `Not Used` |
    `ID` | ID | `0` |
    `IsDynamicCodec` | True or False | `0` |
    `_cachedNotify_` | Cached Notify | `Profiles` |
    `MaxPayloadSize` | Maximum Payload Size (ms) | `30` | `10`, `20`, `30`
    `PayloadDesc` | Payload Description |  |
    `_position_` | _position_ |  |
    `DefaultPayloadType` | Default Payload Type | `Not Used` |
    `SecondaryCodec` | 1 or 0 | `0` |

    #channel_group

    This is a child of `channel_group_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_objectName_` | _objectName_ | `ChannelGroup0 - ID: 0` |
    `OverlapEnable` | Overlap Enable | `Disabled` | `Disabled`, `Enabled`
    `SignalingType` | Signaling Type | `SS7_ISUP` | `SS7_ISUP`, `ISDN`, `SIP`, `H323`
    `CPNCPCRetrievalViaINRINF` | CPN/CPC retrieval via INR/INF | `Disabled` |
    `TBCT` | Channel Transfer | `Disabled` | `Disabled`, `Enabled`
    `MLPP_Support` | Multi-Level Precedence and Preemption (MLPP) Support | `Not Used` |
    `OutTreatment` | Outgoing Treatment | `Release w/Cause` | `None`, `Release w/Cause`
    `InIPProfileId` | Incoming IP Profile ID |  |
    `TermDigit` | Termination Digit | `Not Used` |
    `InterSamTimeout` | Inter SAM Timeout (Seconds) | `15` |
    `_position_` | _position_ |  |
    `InRouteTable` | Route Table | `None` |
    `UnknownTLV2` | UnknownTLV2 | `11` |
    `ID` | ID | `0` |
    `_cached_` | Cached |  |
    `TxmtGain` | Transmit Gain | `0 dB` | `-21 dB`, `-18 dB`, `-15 dB`, `-12 dB`, `-9 dB`, `-6 dB`, `-3 dB`, `0 dB`, `3 dB`, `6 dB`, `9 dB`, `12 dB`, `15 dB`, `18 dB`
    `OutIPProfile` | Outgoing IP Profile | `Not Used` |
    `_cachedNotify_` | Cached Notify | `ChannelGroups` |
    `UnknownTLV1` | UnknownTLV1 | `21` |
    `RcvGain` | Receive Gain | `0 dB` | `-21 dB`, `-18 dB`, `-15 dB`, `-12 dB`, `-9 dB`, `-6 dB`, `-3 dB`, `0 dB`, `3 dB`, `6 dB`, `9 dB`, `12 dB`, `15 dB`, `18 dB`
    `InTreatment` | Incoming Treatment | `Release w/Cause` |
    `OutHunting` | Hunting Options | `Round Robin Clockwise` | `Alternate Even`, `Alternate Odd`, `LRU`, `Most Idle`, `Round Robin Clockwise`, `Round Robin Counter Clockwise`, `Sequential Bottom Up`, `Sequential Top Down`
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `Name` | Name | `ChannelGroup0` |
    `OutTransTable` | Outgoing Translation Table | `None` |
    `ReCauseCode` | Re-Attempt Cause Code | `Not Used` | `Not Used`, `000 - Reserved`, `001 - Unallocated`, `002 - No Route to Specified Transit Network`, `003 - No Route to Destination`, `004 - Send Special Information Tone`, `005 - Misdialled Trunk Prefix`, `006 - Channel Unacceptable`, `007 - Call Awarded`, `008 - Preemption`, `009 - Preemption - Circuit Reserved for Reuse`, `010 - Unknown Cause Code`, `011 - Unknown Cause Code`, `012 - Unknown Cause Code`, `013 - Unknown Cause Code`, `014 - Unknown Cause Code`, `015 - Unknown Cause Code`, `016 - Normal Call Clearing`, `017 - User Busy`, `018 - No User Responding`, `019 - No Answer from User`, `020 - Subscriber absent`, `021 - Call Rejected`, `022 - Number Changed`, `023 - Unknown Cause Code`, `024 - Unknown Cause Code`, `025 - Exchange routing error`, `026 - Non-Selected User Clearing`, `027 - Destination Out of Order`, `028 - Invalid Number Format`, `029 - Facility Rejected`, `030 - Response to STATUS ENQUIRY`, `031 - Normal Unspecified`, `032 - Unknown Cause Code`, `033 - Unknown Cause Code`, `034 - No Circuit/Channel Available`, `035 - Unknown Cause Code`, `036 - Unknown Cause Code`, `037 - Unknown Cause Code`, `038 - Network Out of Order`, `039 - Frame Mode Connection Out of Service`, `040 - Frame Mode Connection Operational`, `041 - Temporary Failure`, `042 - Switching Equipment Congestion`, `043 - Access Information Discarded`, `044 - Requested Circuit/Channel Unavailable`, `045 - Unknown Cause Code`, `046 - Precedence Call Blocked`, `047 - Resource Unavailable unspecified`, `048 - Unknown Cause Code`, `049 - Quality of Service Unavailable`, `050 - Requested Facility Not Subscribed`, `051 - Unknown Cause Code`, `052 - Unknown Cause Code`, `053 - Outgoing Calls Barred Within CUG`, `054 - Unknown Cause Code`, `055 - Incoming Calls Barred Within CUG`, `056 - Unknown Cause Code`, `057 - Bearer Capability Not Authorized`, `058 - Bearer Capability Not Available`, `059 - Unknown Cause Code`, `060 - Unknown Cause Code`, `061 - Unknown Cause Code`, `062 - Inconsistency b/w access info and sub class`, `063 - Service of Option Not Available unspecified`, `064 - Unknown Cause Code`, `065 - Bearer Capability Not Implemented`, `066 - Channel Type Not Implemented`, `067 - Unknown Cause Code`, `068 - Unknown Cause Code`, `069 - Requested Facility Not Implemented`, `070 - Restricted Digital Info Bearer Only`, `071 - Unknown Cause Code`, `072 - Unknown Cause Code`, `073 - Unknown Cause Code`, `074 - Unknown Cause Code`, `075 - Unknown Cause Code`, `076 - Unknown Cause Code`, `077 - Unknown Cause Code`, `078 - Unknown Cause Code`, `079 - Service or Option Not Implemented unspecified`, `080 - Unknown Cause Code`, `081 - Invalid Call Reference Value`, `082 - Identified Channel Does Not Exist`, `083 - Call Identity Does Not Exist`, `084 - Call Identity In Use`, `085 - No Call Suspended`, `086 - Call Identity Has Been Cleared`, `087 - User Not Memeber of CUG`, `088 - Incompatible Destination`, `089 - Unknown Cause Code`, `090 - Non-existent CUG`, `091 - Invalid Transit network Selection`, `092 - Unknown Cause Code`, `093 - Unknown Cause Code`, `094 - Unknown Cause Code`, `095 - Invalid Message unspecified`, `096 - Mandatory Information Element Missing`, `097 - Message Type Non-existent or Not Implemented`, `098 - Message Not Compatible with Call State`, `099 - Information Element/Parameter Non-existent`, `100 - Invalid Information Element Contents`, `101 - Message Not Compatible with Call State`, `102 - Recovery on Timer Expired`, `103 - Parameter Non-existent or Not Implemented`, `104 - Unknown Cause Code`, `105 - Unknown Cause Code`, `106 - Unknown Cause Code`, `107 - Unknown Cause Code`, `108 - Unknown Cause Code`, `109 - Unknown Cause Code`, `110 - Message with Unrecognized Parameter`, `111 - Protocol Error unspecified`, `112 - Unknown Cause Code`, `113 - Unknown Cause Code`, `114 - Unknown Cause Code`, `115 - Unknown Cause Code`, `116 - Unknown Cause Code`, `117 - Unknown Cause Code`, `118 - Unknown Cause Code`, `119 - Unknown Cause Code`, `120 - Unknown Cause Code`, `121 - Unknown Cause Code`, `122 - Unknown Cause Code`, `123 - Unknown Cause Code`, `124 - Unknown Cause Code`, `125 - Unknown Cause Code`, `126 - Unknown Cause Code`, `127 - Unknown Cause Code`, `128 - Unknown Cause Code`, `129 - Unknown Cause Code`, `130 - Unknown Cause Code`, `131 - Unknown Cause Code`, `132 - Unknown Cause Code`, `133 - Unknown Cause Code`, `134 - Unknown Cause Code`, `135 - Unknown Cause Code`, `136 - Unknown Cause Code`, `137 - Unknown Cause Code`, `138 - Unknown Cause Code`, `139 - Unknown Cause Code`, `140 - Unknown Cause Code`, `141 - Unknown Cause Code`, `142 - Unknown Cause Code`, `143 - Unknown Cause Code`, `144 - Unknown Cause Code`, `145 - Unknown Cause Code`, `146 - Unknown Cause Code`, `147 - Unknown Cause Code`, `148 - Unknown Cause Code`, `149 - Unknown Cause Code`, `150 - Unknown Cause Code`, `151 - Unknown Cause Code`, `152 - Unknown Cause Code`, `153 - Unknown Cause Code`, `154 - Unknown Cause Code`, `155 - Unknown Cause Code`, `156 - Unknown Cause Code`, `157 - Unknown Cause Code`, `158 - Unknown Cause Code`, `159 - Unknown Cause Code`, `160 - Unknown Cause Code`, `161 - Unknown Cause Code`, `162 - Unknown Cause Code`, `163 - Unknown Cause Code`, `164 - Unknown Cause Code`, `165 - Unknown Cause Code`, `166 - Unknown Cause Code`, `167 - Unknown Cause Code`, `168 - Unknown Cause Code`, `169 - Unknown Cause Code`, `170 - Unknown Cause Code`, `171 - Unknown Cause Code`, `172 - Unknown Cause Code`, `173 - Unknown Cause Code`, `174 - Unknown Cause Code`, `175 - Unknown Cause Code`, `176 - Unknown Cause Code`, `177 - Unknown Cause Code`, `178 - Unknown Cause Code`, `179 - Unknown Cause Code`, `180 - Unknown Cause Code`, `181 - Unknown Cause Code`, `182 - Unknown Cause Code`, `183 - Unknown Cause Code`, `184 - Unknown Cause Code`, `185 - Unknown Cause Code`, `186 - Unknown Cause Code`, `187 - Unknown Cause Code`, `188 - Unknown Cause Code`, `189 - Unknown Cause Code`, `190 - Unknown Cause Code`, `191 - Unknown Cause Code`, `192 - Unknown Cause Code`, `193 - Unknown Cause Code`, `194 - Unknown Cause Code`, `195 - Unknown Cause Code`, `196 - Unknown Cause Code`, `197 - Unknown Cause Code`, `198 - Unknown Cause Code`, `199 - Unknown Cause Code`, `200 - Unknown Cause Code`, `201 - Unknown Cause Code`, `202 - Unknown Cause Code`, `203 - Unknown Cause Code`, `204 - Unknown Cause Code`, `205 - Unknown Cause Code`, `206 - Unknown Cause Code`, `207 - Unknown Cause Code`, `208 - Unknown Cause Code`, `209 - Unknown Cause Code`, `210 - Unknown Cause Code`, `211 - Unknown Cause Code`, `212 - Unknown Cause Code`, `213 - Unknown Cause Code`, `214 - Unknown Cause Code`, `215 - Unknown Cause Code`, `216 - Unknown Cause Code`, `217 - Unknown Cause Code`, `218 - Unknown Cause Code`, `219 - Unknown Cause Code`, `220 - Unknown Cause Code`, `221 - Unknown Cause Code`, `222 - Unknown Cause Code`, `223 - Unknown Cause Code`, `224 - Unknown Cause Code`, `225 - Unknown Cause Code`, `226 - Unknown Cause Code`, `227 - Unknown Cause Code`, `228 - Unknown Cause Code`, `229 - Unknown Cause Code`, `230 - Unknown Cause Code`, `231 - Unknown Cause Code`, `232 - Unknown Cause Code`, `233 - Unknown Cause Code`, `234 - Unknown Cause Code`, `235 - Unknown Cause Code`, `236 - Unknown Cause Code`, `237 - Unknown Cause Code`, `238 - Unknown Cause Code`, `239 - Unknown Cause Code`, `240 - Unknown Cause Code`, `241 - Unknown Cause Code`, `242 - Unknown Cause Code`, `243 - Unknown Cause Code`, `244 - Unknown Cause Code`, `245 - Unknown Cause Code`, `246 - Unknown Cause Code`, `247 - Unknown Cause Code`, `248 - Unknown Cause Code`, `249 - Unknown Cause Code`, `250 - Unknown Cause Code`, `251 - Unknown Cause Code`, `252 - Unknown Cause Code`, `253 - Unknown Cause Code`, `254 - Unknown Cause Code`
    `TotalSamTimeout` | Total Overlap Timeout (Seconds) | `18` |
    `ResourceGroupId` | ResourceGroupId | `0` |
    `GroupFunction` | Trunk Direction | `Incoming/Outgoing` | `Incoming/Outgoing`, `Incoming`, `Outgoing`
    `InIPProfile` | Incoming IP Profile | `Not Used` |
    `OutCallProgressTones` | Ingress Side will Play Call Progress Tones | `False` | `True`, `False`
    `MinDigits` | Minimum # of Digits | `Not Used` |
    `NetworkElementId` | NetworkElementId |  |
    `SupportA2F` | Support Digit A to F | `False` | `True`, `False`
    `InTransTable` | Incoming Translation Table | `None` |
    `INCCTable` | Cause Code Table | `None` |

    #signaling

    This is a child of `bn2020`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_position_` | _position_ |  |
    `_objectName_` | _objectName_ | `Signaling` |

    #ip_address

    This is a child of `interface`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `NIIPIcmpSupport` | ICMP | `Enable` | `Disable`, `Enable`
    `ConfigTableID` | Table Id | `0x0020` |
    `NodeName` | NodeName |  |
    `NIIPAddress` | IP Address |  |
    `NIIPSubnet` |  / Network Prefix Len | `24` |
    `VLanID` | VLAN ID (2-4094) | `2` |
    `SiblingIPType` | SiblingIPType |  |
    `VLanPriority` | VLAN Priority (0-7) | `0` |
    `NIIPArpSupport` | ARP/ND | `Enable` | `Disable`, `Enable`
    `NIIPPhy` | Source Endpoint | `Services` | `Services`, `Media 0`, `Media 1`
    `ConfigAction` | Activate | `Enable` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `FQDN` | FQDN (SIP Only) |  |
    `_objectName_` | _objectName_ | `Services -  / 24 ` |
    `MaxPrefixLength` | Max Prefix Length | `32` |
    `NIIPLogical` | Logical Interface |  |
    `NIIPGateway` | Default Gateway |  |
    `NIIPType` | Address Type | `IPv4` | `IPv4`, `IPv6`
    `VLan` | VLAN | `Disable` | `Disable`, `Enable`
    `ACLName` | ACL | `Unrestricted` |
    `MinPrefixLength` | Min Prefix Length | `1` |
    `_position_` | _position_ |  |

    #facility

    This is a child of `bn2020`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `QryFrq_SyncMode` | Monitor Refresh Rate (Seconds) | `10` |
    `_objectName_` | _objectName_ | `Facility` |
    `_position_` | _position_ |  |

    #channel_group_collection

    This is a child of `routing_configuration`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_position_` | _position_ |  |
    `_objectName_` | _objectName_ | `Channel Groups` |
    `ResourceGroup` | ResourceGroup | `Resource Group` |
    `IpRouterTable` | IpRouterTable | `IP Router Table` |
    `_cached_` | Cached | `__NULL__` |

    #sip_ip

    This is a child of `sip`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `TransportType` | Transport Type | `UDP` | `UDP`, `TCP`, `TLS`
    `IPType` | IP Type | `IPv4` | `IPv4`, `IPv6`
    `ID` | ID | `0` |
    `DefaultSecureProfile` | Default Secure Profile | `Not Used` |
    `_position_` | _position_ |  |
    `SecureProfileID` | Secure Profile ID | `Not Used` |
    `DNSClient` | DNS Client | `Not Used` |
    `NodeName` | NodeName |  |
    `TLSPort` | TLS Port | `5061` |
    `SecureProfile` | Secure Profile | `Not Used` |
    `FQDN` | Fully Qualified Domain Name |  |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `DNSQueryMode` | DNS Query Mode | `MIX` | `MIX`, `A ONLY`, `SRV ONLY`
    `IPAddress` | IP Address |  |
    `Port` | Port | `5060` |
    `DefaultSecureProfileID` | Default Secure Profile ID | `Not Used` |
    `_objectName_` | _objectName_ | `SIP IP Address: ` |
    `DNSClientID` | DNSClient ID | `Not Used` |

    #packet_facility

    This is a child of `packet_facility_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `NetworkAddress` | Network Address |  |
    `EndSpanID` | End Span | `0` |
    `_position_` | _position_ |  |
    `GroupID` | ID | `1` |
    `EndChannelID` | End Channel | `31` |
    `_cachedNotify_` | Cached Notify | `ChannelGroups` |
    `StartSpanID` | Start Span | `0` |
    `RTPOffset` | Starting RTP Port |  |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `FQDN` | FQDN (Media) |  |
    `_objectName_` | _objectName_ | `PacketFacility - Packet_Facility1` |
    `AddressType` | Address type | `0` |
    `MediaTLV` | MediaTLV |  |
    `ChannelType` | Packet Facility Channel Type |  |
    `GroupName` | Name | `Packet_Facility1` |
    `StartChannelID` | Start Channel | `0` |
    `ChannelCount` | Number of Channels |  |
    `MediaEndpoint` | Media Endpoint |  |
    `NodeName` | NodeName |  |

    #external_network_elements

    This is a child of `root`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_position_` | _position_ |  |
    `_objectName_` | _objectName_ | `External Network Elements` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |

    #sip

    This is a child of `signaling`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `SIPTEnabled` | SIP-T Enabled | `No` | `No`, `Yes`
    `Variant` | Variant |  |
    `RoutingMethod` | Routing Method | `0x08` |
    `_objectName_` | _objectName_ | `SIP` |
    `SIPTBehaviour` | SIP-T Behavior | `Not Used` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `RetryAfter` | Retry-After (# of Seconds) | `5` |
    `VirtualAddress` | Virtual Address |  |
    `RouterProtocolId` | Router Protocol Id | `0x0B` |
    `IPOperationMode` | IP Operation Mode | `Single IP` | `Single IP`, `Multiple IP`
    `AddrOfRecord` | UserName (AOR) | `DIALOGIC-BDN__NOTFOUND__` |
    `AuthPassword` | Authentication Password |  |
    `TotalSamTimeout` | Total Overlap Timeout |  |
    `VariantId` | VariantId |  |
    `InterSamTimeout` | Inter SAM Timeout |  |
    `_position_` | _position_ |  |
    `_cached_` | Cached |  |
    `SIPMsgRestriction` | Message Restriction Setting | `Default` | `Default`, `Option 1`
    `Node` | Node |  |
    `CompactHeader` | Compact Header | `Disable` | `Disable`, `Enable`
    `AuthUserName` | Authentication User Name |  |
    `RoutingCriteriaType` | RoutingCriteriaType | `0x2792` |

    #interface

    This is a child of `interface_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `Interface` | Interface | `Control` | `Control`, `Data A`, `Data B`
    `ConfigTableId` | Config Table Id | `0x1303` |
    `QryFrq_NetLogIntfc` | Monitor Refresh Rate (Seconds) | `10` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `OpTableId` | Operation Table Id | `0x1306` |
    `_position_` | _position_ |  |
    `_objectName_` | _objectName_ | `Control` |
    `MonitorTableId` | Monitor Table Id | `0x1305` |

    #node_association

    This is a child of `cg_network_element`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `IPAddress` | Service IP Address |  |
    `Port` | Port |  |
    `_objectName_` | _objectName_ | `Node Assoc: ` |
    `PacketFacilityId` | PacketFacilityId |  |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `UnknownTLV1` | UnknownTLV1 | `21` |
    `DNSClientID` | DNSClient ID |  |
    `DNSClient` | ENUM Client |  |
    `IPAddress4` | Service IP Address |  |
    `_position_` | _position_ |  |
    `HostName` | HostName | `Not Used` |
    `UnknownTLV2` | UnknownTLV2 | `11` |
    `SetID` | SetID |  |
    `_cachedNotify_` | Cached Notify | `ChannelGroups` |
    `NetworkElement` | NetworkElement |  |
    `TransportType` | TransportType |  |
    `PacketFacility` | Media Packet Facility |  |
    `Node` | Node |  |

    #external_gateway

    This is a child of `external_gateway_collection`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `SecureProfile` | Secure Profile | `Not Used` |
    `TransportTypeId` | TransportTypeId | `0x00` |
    `Name` | Name |  |
    `MaxGWPrefix` | MaxGWPrefix | `32` |
    `IPAddress4` | IP Address |  |
    `Registration` | Registration Required | `No` | `No`, `Yes`
    `AllowedGWPrefix` | Allowed Gateway Subnet Prefix | `32` |
    `ProtocolId` | ProtocolId | `0x02` |
    `PPLComponentId` | PPLComponentId | `213` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `SGPId` | SIP Profile Id |  |
    `RegistrationExpire` | Registration Interval | `3600` |
    `_objectName_` | _objectName_ |  |
    `AddressType` | Address Type | `IP Address` | `IP Address`, `Host Name`
    `Port` | Transport Port | `5060` |
    `IPAddress` | IP Address |  |
    `KeepAlive` | OPTIONS Keep Alive | `Disable` | `Disable`, `Enable`
    `Protocol` | Protocol | `SIP` | `SIP`, `H323`
    `NetworkName` | NetworkName | `GW: ` |
    `ID` | ID | `1024` |
    `IPType` | IP Type | `IPv4` | `IPv4`, `IPv6`
    `TransportType` | Transport Type | `UDP` | `UDP`, `TCP`, `TLS`
    `_cachedNotify_` | Cached Notify | `ChannelGroups` |
    `SecureProfileID` | Secure Profile ID | `Not Used` |
    `SGP` | Profile |  |
    `KeepHostName` | Keep HostName in outgoing SIP request | `Disabled` | `Disabled`, `Enabled`
    `ElementType` | ElementType |  |
    `HostName` | HostName |  |
    `_position_` | _position_ |  |

    #bn2020

    This is a child of `root`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `SwVersion` | Software Version | `Unknown` |
    `LicIPChannels` | Total Licensed IP Channels | `0` |
    `ResendLogic` | Resend Logic | `Disable` | `Disable`, `Resend Once`, `Once With Alarm`, `Until Acked`
    `Name` | Name | `Node0` |
    `CFCMode` | Trunk Type | `Unknown` | `T1`, `E1`, `Unknown`
    `PacketAudioChannels` | Packet Audio Channels | `Unknown` |
    `IPAddress` | IP Address (nn.nn.nn.nn) |  |
    `_objectName_` | _objectName_ | `BN2020: Node0 - ID: 0` |
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `IPChannels` | Total IP Channels | `Unknown` |
    `NetworkMultimediaChannels` | Network Multimedia Channels | `Unknown` |
    `srtpEnable` | Audio SRTP Support | `Disabled` | `Disabled`, `Enabled`
    `MediaMode` | Media Mode | `Audio LBR` | `Audio LBR`, `Audio 3G`, `Audio HD`, `Audio Dynamic Density Management`, `Multimedia - [Video:  0 percent TransCode]`, `Multimedia - [Video: 25 percent TransCode]`, `Multimedia - [Video:100 percent TransCode]`
    `InterfaceType` | Interface Type | `Unknown` | `DS-3/OC3`, `DS-1`, `Unknown`
    `NodeType` | Type | `Unknown` | `2020`, `Unknown`
    `IPType` | IP Type | `IPv4` |
    `ID` | ID | `0` |
    `ACL_ID` | ACL ID | `0` |
    `_position_` | _position_ |  |
    `PacketMultimediaChannels` | Packet Multimedia Channels | `Unknown` |
    `ACLName` | ACL | `Unrestricted` |
    `SubNetMask` | SubNet Mask |  |

    #route_table_collection

    This is a child of `routing_configuration`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_objectName_` | _objectName_ | `Routing Tables` |
    `_position_` | _position_ |  |

    #interface_collection

    This is a child of `network`

    ## Options

    Name|Description|Default|Alternatives
    ----|-----------|-------|------------
    `_localDbSyncKey_` | _localDbSyncKey_ | `0` |
    `_objectName_` | _objectName_ | `Logical Interfaces` |
    `_position_` | _position_ |  |